The access layer

Ethernet switches video

.

MAC address tables video

How a switch learns PC’s MAC addresses